INFRALAN® LC couplings in plastic housing

INFRALAN® LC couplings in plastic housing,

The INFRALAN® LC Duplex coupling in a coloured plastic housing according to fibre class OM5 for SC-Simplex break-outs complies with DIN EN 61754-20. Due to the one-piece design, it has a higher stability and a low sensitivity to temperature fluctuations. Mounting options are available via clips or enclosed ST2.5 self-tapping screws, including dust protection caps.

Connector type 1st side: LC Duplex

Connector type 2. side: LC Duplex

Colour: lime green

Material: plastic

Type of mounting: screw/engagement

Sleeve material: Ceramic

Design: SC-Simplex

Operating temperature: -40 to 85°C

Storage temperature: -40 to 85°C

Dimensions: hxbxt 9,3x22x29,2mm

Make: INFRALAN®

Item no.: IKL-LCDU-MM-K-LG