INFRALINFRALAN® Consolidation Point Cable PVS

INFRALAN® Consolidation Point Cable PVS,

consists of three following components of the INFRALAN® program:

INFRALAN® RJ45 slimline connection module Cat.6a (IKS-6A-PVP-XX), INFRALAN® Cat.7 component certified by GHMT according to Premium Verification Program (PVP) Laying cable S/FTP 1000 MHz CPR Cca as simplex cable with 4x2xAWG23/1 with PVP certification of the GHMT (99981.x-CPR) and the INFRALAN® Cat.6A field assembly RJ45 connector STP (IVB-6A-S).

These are combined in one cable and thus offer a flexible variant for producing a 4 connector link.

Category: 6A

Application: 10 Gigabit Ethernet

Plug connector 1st side: RJ45 plug IVB-6A-S

Connector 2nd side: RJ45 Keystone IKS-6A-PVP-XX

Coat colour: orange

Flame resistance according to: EN60332-3-24

Length: 5,0m

Make: INFRALAN®

Item no.: ICP-6A-PVS-0500

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

INFRALAN® Consolidation Point Cable PVS

INFRALAN® Consolidation Point Cable PVS,

as described above, however:

Length: X,Xm

Make: INFRALAN®

Item no.: ICP-6A-PVS-XXXX

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Structure Art. no:

ICP-6A-PVS-XXXX

 -XXXX = Length = "0500" = 5,0m

Available in lengths:

5,00m / 10,00m / 15,00m

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Structure Art. no:

ICP-6A-KOP-XXXX

 -XXXX = Length = "0500" = 5,0m

Available in lengths:

5,00m / 10,00m / 15,00m