INFRALAN® SC coupling in plastic housing

INFRALAN® SC coupling in plastic housing,

The INFRALAN® SC Duplex coupling in a coloured plastic housing according to fibre class OM5 complies with DIN EN 61754-4. Mounting options are via clips or enclosed ST2.5 self-tapping screws, incl. dust protection caps.

Connector type 1st side: SC Duplex

Connector type 2. side: SC Duplex

Colour: lime green

Material: plastic

Type of mounting: screw/engagement

Sleeve material: Ceramic

Design: SC-Duplex

Operating temperature: -40 to 75°C

Storage temperature: -40 to 85°C

Dimensions: hxbxt 9,4x34,7x27,4mm

Make: INFRALAN®

Item no.: IKL-SCDU-MM-K-LG